---Residual stress measurements---

    - the specimen numbers are assigned the load cycles in "specimen_loadCycles.xlsx"
    - drilling cutter with 1,6mm diameter
    - air turbine drilling motor with 200,000 1/min