---Initial bending---

    - specimen #0007 and specimen #0124 are included
    - a single loading and unloading was carried out
    - ARAMIS DIC data is in .csv file format
        + each .csv file (except <common.csv>) corresponds to a time step during experiment
        + in each .csv file the information is saved layerwise, i.e. for discrete y coordinate values. That was done for an evaluation as averaged strain profile over the domain with constant bending moment.
        + <common.csv> contains the machine data for force and displacement of the hydraulic cylinder and the rotation of the support structures used (see test setup and corresponding paper)
    - some of the naming is unfortunately in german (use translator if necessary)