### Element geometries ###

# Reinforcement, Diameter 8 cm #
Name: D8
Cross-section input: Diameter 
Diameter of bar: 0.008

# Reinforcement, Diameter 10 cm #
Name: D10
Cross-section input: Diameter 
Diameter of bar: 0.01

# Reinforcement, Diameter 12 cm #
Name: D12
Cross-section input: Diameter
Diameter of bar: 0.012

# Reinforcement, Diameter 14 cm #
Name: D14
Cross-section input: Diameter 
Diameter of bar: 0.014

# Reinforcement, Diameter 16 cm #
Name: D16
Cross-section input: Diameter 
Diameter of bar: 0.016

# welded Reinforcement Mesh #
Name: POS_1-Matte_Q636A
Thickness: Diameter and spacing
Diameter of bars oriented in local x direction: 0.01
Diameter of bars oriented in local y direction: 0.009
Spacing between bars oriented in local x direction: 0.1
Spacing between bars oriented in local y direction: 0.125
Reinforcement x axis: [1 0 0]

# Prestressing steel - bonded post-tensioning tendons #
Name: Prestressing steel - bonded post-tensioning tendons 
Cross-section input: Cross-section
Cross-section area of bar: 0.0006

# Prestressing steel - pre-tensioning #
Name: Prestressing steel - pre-tensioning
Cross-section input: Cross-section
Cross-section area of bar: 9.3e-05






