### Loads ###

# Dead loads #
Name: Dead loads
(1)
Name: Deadweight
Load type: Deadweight
(2) 
Name: Prestressing bonded post-tensioning tendons FT1.1
Load target type: Shape
Load type: Reinforcement bar prestress
Loaded wires: FT1.1-SPS-nV-Polylinie
Prestress in bar: 1.50487e+09
(3)
Name: Prestressing bonded post-tensioning tendons FT2.1
Load target type: Shape
Load type: Reinforcement bar prestress
Loaded wires: FT2.1-SPS-nV-Polylinie
Prestress in bar: 1.43576e+09
(4)
Name: Prestressing pre-tensioning
Load target type: Shape
Load type: Reinforcement bar prestress
Loaded wires: all Prestressing pre-tensioning Tendons 
Prestress in bar: 1.30108e+09

# Load test #
Name: Area Load
Load target type: Face
Load type: Distributed force
Loaded face: Face of OB-Span2
Face force value: -1.75e+07
Force load direction: Z 
Comment: In order to apply an area load on the face of OB-Span2 with dimensions of 20 × 20 cm, a sheet must first be projected.
Sheet: [ [ 27.05, 4.045, 3.59 ], [ 27.25, 4.045, 3.59 ], [ 27.25, 4.245, 3.59 ], [ 27.05, 4.245, 3.59 ] ]




